|  |  |  |
| --- | --- | --- |
| **Site** | **Location** | **Description** |
| Earth Dam | Pacific rd | check spillway |
| Upper Level of One Mile Creek. Dam to Beach rd | Pacific Rd to Beach Rd | check for blockages and clear if necessary |
| One Mile creek | 11 Beach rd | check sand level, open or closed, check for other debris and clear if necessary |
| Jenkinson st | 12 Jenkinson st | check outlet structure and trash catcher, and clear if necessary |
| 54 Beach Rd | 54 Beach Rd | check culvert under rd, and inside box culvert for blockages, clear if necessary |
| Browns drive pond outlet | Outlet structure, feeding Maranui pond, opposite 23 Browns drive | check grill for blockage, clear if needed, comment on silt in pond |
| Maranui pond outlet | 91 Beach rd | check outlet structure, grill and scruffy dome, clear if necessary |
| 94 Beach Rd  | House at end of drive | Check grill far coner of section |
| Darley Drain | Ocean view rd/savage ave | check for blockages, ( logs etc) and clear if necessary |
| Storm water pump station | 37 Shaw rd | check operation of pumps, check flow visable at outlet in coronation park, check for blockages, clear if necessary, check trash catcher in well |
| Two Mile Creek | Dillon st/ Seaforth rd | check sand level(open or closed) check gauge on bridge, record, check for other debris(logs etc) clear if necessary |
| seaforth rd outlet into 2 mile creek | Between #1 seaforth rd and 2 Wilson rd | check for blockages and clear if necessary |
| Three mile creek | Seaforth rd near Glen Isla place | check sand Level (open or closed) check gauge on bridge, record, check for other debris( logs etc) clear if necessary |
| Storm water pump station | Marlin Ave(cnr 66 Broadway | check operation of pumps, check flow is visable at receiving manhole in rd near 266 Seaforth rd, clear any blockages |
| Storm water pump station | 9 Papuanahi rd | check operation of pump, check flow visable at outlet in sand dunes, clear around outlet if necessary |
| Swale and Outlet behind 477 Seaforth rd | behind 477 Seaforth | check outlet from swale, access from Bowentown blvd, clear grill if necessary |
| Storm water pump station | Opposite #10 Bowentown Blvd | check operation of pump, check flow visable at outlet in sand dunes, clear around outlet if necessary |
| Storm water pump station | 56 Bowentown blvd | check operation of pump, check flow visable at outlet in sand dunes, clear around outlet if necessary |
| Otawhiwhi Marae inlet structure | 452 Seaforth rd | check outlet to drain for blockage, clear if necessary, do not go behind Marae Fence |
| Storm water pump station | 449 Seaforth rd | check operation of pump, check flow is visable at outlet outside Marae fence, clear any blockages |
| Storm water pump station | Pio rd/Tatai Rd | check operation of pump, check flow at outlet to pond at seaforth rd/pio rd cnr, clear any blockages, including grill into pump station |